4WD CONTROL MODULE REMOVAL/INSTALLATION

id031800806000

1. For L.H.D., remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

2. For R.H.D., remove the following parts:

  (1) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

  (3) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

ac9uuw00001403

1 | Bolt
2 | 4WD CM (See 4WD CM Removal Note.)
3 | Connector

4WD CM Removal Note

1. Push up the 4WD CM slightly, and remove it.

ac9wzw00000121