SIDE SILL PANEL REMOVAL [PANEL REPLACEMENT]

id098008743700

1. Rough cut area (A), drill the 129 locations indicated by (B), and then remove the side sill (outer).

  Note
  • Chisel is inserted because the laser welding is given as for the arrow part of the figure below and the welding is separated.

ac9wzb00000005

2. Rough cut area (C).

  Caution
  • During rough cutting, be careful not to damage the hinge reinforcement and the center pillar reinforcement (inner) indicated by dotted lines in the figure.

3. Drill the 3 locations indicated by (D) from the interior.

4. Remove the side sill reinforcement.

ac9wzb00000006