CLEARING DTC [INSTRUMENT CLUSTER]

id0902e8400300

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “IC”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Turn the ignition switch to the OFF position.

6. Turn the ignition switch to the ON position and wait for 5 s or more.

7. Perform DTC inspection. (See DTC INSPECTION [INSTRUMENT CLUSTER].)

8. Verify that no DTCs are displayed.