OIL PUMP DISASSEMBLY/ASSEMBLY [AY6A-EL, AY6AX-EL]

id0517k3332700

  Note
  • The following procedure is for replacement of the O-ring and seal rings only. Replace the transaxle if other repairs are necessary.

1. Disassemble in the order indicated in the figure.

2. Assemble in the reverse order of disassembly.

ac9uuw00004043

1 | O-ring (See O-ring Disassembly Note.) (See O-ring Assembly Note.)
2 | Seal ring (See Seal Ring Disassembly Note.) (See Seal Ring Assembly Note.)

O-ring Disassembly Note

1. Remove the O-ring from the oil pump component.

am6xuw00004179

Seal Ring Disassembly Note

1. Remove the seal rings from the oil pump component.

am6xuw00004175

Seal Ring Assembly Note

1. Apply ATF to the new seal rings and sliding surface of the oil pump component.

2. Compress the new seal rings as shown in the figure. Then install the seal rings to the oil pump component.

ac9uuw00004044

  Caution
  • Do not expand the seal rings too much.
  • Be careful not to shorten the seal rings too much, when installing the seal rings.

  Note
  • Verify that oil seal rings rotate smoothly after installing them.

O-ring Assembly Note

1. Apply ATF to a new O-ring.

2. Install the new O-ring to the oil pump component.

ac9uuw00004045