SUNROOF UNIT REMOVAL/INSTALLATION

id091500800700

  Caution
  • If the sunshade is forced close while the sunroof is open, the sunshade could be damaged.

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (6) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (8) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (9) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

  (14) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (15) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (18) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (19) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (20) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (21) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (22) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

3. Remove the sunroof seaming welt.

4. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION.)

5. Remove the glass panel (See GLASS PANEL REMOVAL/INSTALLATION.)

6. Disconnect the front and rear drain hose from the sunroof frame.

7. Remove the bolts.

ac9wzw00001568

8. Remove the nuts, and then remove the sunroof unit.

9. Install in the reverse order of removal.

10. Adjust the glass panel. (See GLASS PANEL ADJUSTMENT.)