DASHBOARD GARNISH REMOVAL/INSTALLATION

id091700804700

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

3. Remove the screw.

ac9uuw00000306

4. Detach clips A by pulling them in the direction of the arrow.

5. Remove the dashboard garnish.

6. Install in the reverse order of removal.