BRAKE SPECIFICATIONS

id040000100300

Item | Specification
--- | ---
Brake pedal | Type | Suspended design
Pedal lever ratio | 2.9
Max. stroke | (mm {in}) | 130.5 {5.138}
Master cylinder | Type | Tandem
Cylinder bore | (mm {in}) | 22.2 {0.874}
Front brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 45.4 {1.79}× 2
Pad dimensions (area x thickness) | 6,000 × 12.0 {9.300 × 0.47}
(mm2 x mm {in2 x in})
Disc plate dimensions | (mm {in}) | 320 × 28 {12.6 × 1.1}
Rear brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 42.85 {1.687}
Pad dimensions (area x thickness) | 3,300 × 11 {5.115 × 0.43}
(mm2 x mm {in2 x in})
Disc plate dimensions | (mm {in}) | 325 × 18 {12.8 × 0.71}
Power brake unit | Type | Vacuum multiplier, single diaphragm
Outer diameter | (mm {in}) | 288 {11.3}
Rear wheel braking force control device | Type | Electronic brakeforce distribution (EBD)
Brake piping | Piping layout | X pattern
Parking brake | Type | Mechanical design, rear two-wheel braking
Operating method (application/release) | Foot actuated type
Drum brake type | Servo type
Lining dimensions (area x thickness) | 4,700 × 3.4 {7.285 × 0.13}
(mm2 x mm {in2 x in})
Drum inner diameter | (mm {in}) | 190 {7.48}
Play adjustment method | Manual-adjusting
Brake fluid | Type | Russian specs.: SAE J1703 or FMVSS116 DOT-3 or DOT-4 Australian, General (L.H.D.) specs.: SAE J1703 or FMVSS116 DOT-3