DRIVELINE/AXLE FEATURES

id030000100100

Improved driveability | • Bell-shaped constant velocity joint adopted for wheel-side joint of front and rear drive shaft • Tripod-shaped constant velocity joint adopted for differential-side joint of front drive shaft • Double offset-shaped constant velocity joint adopted for differential-side joint of rear drive shaft (4WD)
Improved rigidity, reduced noise and vibration | • Characteristics of front drive shaft optimized • Constant velocity joint type rear drive shaft adopted (4WD) • 3-part, 4-joint type propeller shaft with middle shaft bearing has been adopted (4WD)
Improved off-road mobility, handling stability and marketability | • Electronic 4WD control system adopted (4WD)
Size and weight reduction | • Rear differential with an integrated coupling component adopted (4WD) • Aluminum differential carrier adopted (4WD)
Improved serviceability | • Self diagnostic function adopted for electronic 4WD control system (4WD) • A maintenance-free transfer has been adopted (4WD)