DTC C1329, C1330, C1331, C1332, C1333, C1334, C1335, C1336, C1527, C1528, C1530, C1531 [DSC/RSC]

id0402b3811600

DTC | C1329 C1330 C1331 C1332 C1333 C1334 C1335 C1336 C1527 C1528 C1530 C1531 | RF outlet solenoid valve coil system LR outlet solenoid valve coil system RR outlet solenoid valve coil system LF outlet solenoid valve coil system LR inlet solenoid valve coil system LF inlet solenoid valve coil system RF inlet solenoid valve coil system RR inlet solenoid valve coil system RH traction control solenoid valve coil system LH traction control solenoid valve coil system RH stability control solenoid valve coil system LH stability control solenoid valve coil system
DETECTION CONDITION | • Temperature of a solenoid valve coil exceeds specification.
POSSIBLE CAUSE | • This does not indicate a malfunction since constant control over extended period of time is inhibited to protect the RSC solenoid valve inside the DSC/RSC HU

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY DTC TROUBLESHOOTING COMPLETED • Clear the DTC from the memory. (See ON-BOARD DIAGNOSIS [DSC/RSC].) • Are the same DTCs present? | Yes | Replace the DSC/RSC HU/CM, then go to the next step. (See DSC/RSC HU/CM REMOVAL/INSTALLATION [L.H.D.].) (See DSC/RSC HU/CM REMOVAL/INSTALLATION [R.H.D.].)
No | Go to the next step.
2 | VERIFY AFTER REPAIR PROCEDURE • Are any other DTCs present? | Yes | Go to the applicable DTC inspection. (See ON-BOARD DIAGNOSIS [DSC/RSC].)
No | DTC troubleshooting completed.