POWER OUTER MIRROR REMOVAL/INSTALLATION

id091200002400

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Disconnect the power outer mirror connector.

ac9wzw00000837

5. Disconnect the position memory connector.

6. Remove the bolts.

7. Push the power outer mirror against the vehicle and detach the tab while lifting the mirror up to remove.

8. Install in the reverse order of removal.