FOREWORD [RADIO]

id0903e3802700

  Note
  • In case location, time, and broadcasting station etc. can be specified through interview to customer, possibility that signal environment causes problem is high.
  • Perform confirmation of symptom and evaluation under conditions that customer reported (location, time, broadcasting station etc.). If not possible, perform it under equivalent conditions.
  • Before inspection or repair, record the broadcasting stations that customer preset and reset them accordingly after the inspection or repair. Adjust the clock too.

No. | Symptom | Possible DTC
--- | --- | ---
Using the M-MDS | Without using M-MDS (On-board diagnostic test mode)
1 | NO.1 NO RADIO RECEPTION (AM/FM)/NO OR LOW VOLUME [RADIO] | U3003:16, U3000:04 | 09:Er20, 09:Er22
2 | NO.2 NOISE FROM RADIO (AM ONLY) [RADIO] | U3000:04 | 09:Er22
3 | NO.3 NOISE FROM RADIO (FM ONLY) [RADIO] | U3000:04 | 09:Er22
4 | NO.4 CANNOT TUNE (SEEK DOES NOT STOP) [RADIO] | U3003:16, U3000:04 | 09:Er20, 09:Er22
5 | NO.5 CANNOT PRESET (PRESET FUNCTION DOES NOT OPERATE) [RADIO] | — | —
6 | NO.6 RECEPTION FREQUENCY OF RADIO SLIPS [RADIO] | U3000:04 | 09:Er22

Quick Diagnostic Chart

ac9wzw00002917