WHEEL AND TIRE SPECIFICATION

id021200800100

Standard tire

Item | Specification
--- | ---
Tire | Size | 245/60R18 104H | 245/50R20 102V
Air pressure (kPa {bar} <psi>) | Front | 250 {2.5} <36> | 230 {2.3} <33>
Rear
Remaining tread | (mm {in}) | 1.6 {0.07}
Wheel | Size | 18×7 1/2J | 20×7 1/2J
Material | Aluminum alloy
Wheel inset | (mm {in}) | 45 {1.8}
Wheel pitch circle diameter | (mm {in}) | 114.3 {4.5}
Wheel and tire runout | Lateral direction | 2.0 {0.08} max.
(mm {in}) | Radial direction | 1.5 {0.06} max.
Wheel and tire imbalance | (g {oz}) | Adhesive-type*1: 12 {0.42} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max.
*1: Do not install three or more weights. Do not affix the weights such that they are parallel to each other or overlapping. The total weight of all the weights is 160 g {5.64 oz} or less. *2: Do not install three or more weights. One weight is 60 g {2.1 oz} or less and two weights are 100 g {3.53 oz} or less.
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8—147.0 {11.0—14.9, 79.6—108.4}

Spare tire

Item | Specification
--- | ---
Tire | Size | 195/80R17 99M
Air pressure (kPa {bar} <psi>) | 250 {2.5} <36>
Remaining tread | (mm {in}) | 1.6 {0.07}
Wheel | Size | 17×5 1/2J
Material | Steel
Wheel inset | (mm {in}) | 45 {1.8}
Wheel pitch circle diameter | (mm {in}) | 114.3 {4.5}
Wheel and tire runout | Lateral direction | 2.5 {0.09} max.
(mm {in}) | Radial direction | 2.0 {0.07} max.
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8—147.0 {11.0—14.9, 79.6—108.4}