KEYLESS RECEIVER INSPECTION [KEYLESS ENTRY SYSTEM]

id0914008076b3

1. Measure the voltage at the auto light/wiper control module terminals as indicated below.

Terminal Voltage Table (Reference)

ac9wzw00001075

Terminal | Signal name | Connected to | Measured condition | Voltage (V) | Inspection item(s)
--- | --- | --- | --- | --- | ---
A | Power supply | BCM | Under any condition | B+ | • ROOM 15 A fuse • BCM • Related wiring harnesses
D | Serial communication | BCM | Because this terminal is for communication, good/no good judgment by terminal voltage is not possible. | — | • BCM • Related wiring harnesses
E | GND | Body ground | Under any condition. | 1.0 or less | Related wiring harnesses