FRONT HEATER CORE INSPECTION

id071100802300

1. Inspect the front heater core for damage, cracks, and water leakage.

  • If there is any malfunction, replace the front heater core.

2. Visually inspect the fins for bending.

  • If there is any bending, use the end of a flathead screwdriver to straighten the fins.

3. Visually inspect the heater hose for deformation.

  • Repair with pliers if there is deformation. If there is any malfunction, replace the front heater core.