AUTO LEVELING CONTROL MODULE CONSTRUCTION/OPERATION

id091800103800

• In order to prevent blinding from oncoming traffic and to improve visibility, the auto leveling control module automatically controls the optical axis direction for optimal illumination based on signals input from the instrument cluster, auto light/wiper control module and the auto leveling sensor.
• If an error signal from the auto leveling sensor or excessive power supply voltage is detected, the auto leveling indicator light is illuminated to warn the driver of a malfunction.

Optical Axis Adjustment Feature

• The auto leveling control module verifies changes in vehicle speed and attitude based on signal inputted from the instrument cluster, auto light/wiper control module and the auto leveling sensor. The control module then calculates the optimal direction for the optical axis.
• Based on the calculation of the optical axis adjustment amount, the auto leveling control module controls the headlight leveling actuator.

Fail-safe Function

• The fail-safe function operates when the auto leveling control module detects a malfunction. It also warns the driver of a malfunction by illuminating the indicator light as shown in the fail-safe function table.
• The fail-safe function controls each part as shown on the fail-safe function table.

Fail-safe Function Table

Item | Detection item | Fail-safe function | Indicator light | Cancel condition
--- | --- | --- | --- | ---
Auto leveling sensor | Input voltage from headlight auto leveling sensor outside of 0.5 V to 4.5 V range for continuous 10 s period. | Optical axis stopped at current position | Illuminated | Normal value detected for continuous 1 s period
Headlight leveling actuator | Output voltage malfunction (wiring harness wire, short to ground) to headlight leveling actuator. | Optical axis stopped at current position | Illuminated | Normal value detected for continuous 1 s period
Auto leveling control module | Headlight auto leveling system initial setting not implemented | Controls at preset value | Flashes every 0.25 s | Headlight auto leveling system initialization is completed normally

  Note
  • When the ignition switch is turned to the ON position, the auto leveling control module checks the auto leveling indicator light bulb and illuminates the bulb for 3 s to indicate that there is no malfunction.

  ac9wzn00000757