FRONT BUMPER DISASSEMBLY/ASSEMBLY

id091000800400

1. Disassemble in the order indicated in the table.

R.H.D.

ac9wzw00002846

1 | Screw A
2 | Radiator grille
3 | Screw B
4 | Front fog light hole cover
5 | Screw C
6 | Under cover
7 | Nut
8 | Front over fender lower (SeeFront Over Fender Lower Assembly Note.)
9 | Screw D
10 | Licence plate holder
11 | Front bumper face

L.H.D.

ac9wzw00002847

1 | Screw A
2 | Radiator grille
3 | Screw B
4 | Front fog light hole cover
5 | Screw C
6 | Under cover
7 | Nut
8 | Front over fender lower (SeeFront Over Fender Lower Assembly Note.)
9 | Screw D
10 | Licence plate holder
11 | Front bumper face

2. Assemble in the reverse order of disassembly.

Front Over Fender Lower Assembly Note

1. Attach the front over fender lower to the front bumper fascia with nuts.

ac9uuw00000837

2. Use a soldering copper and thermally deform the tab in order to fasten the stiffening rib.