INPUT/TURBINE SPEED SENSOR, VEHICLE SPEED SENSOR (VSS) OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3224700

• The speed sensors are installed in the transaxle case. The input/turbine speed sensor detects the number of revolutions of the intermediate shaft's C2 drum as input shaft speed. The VSS detects the number of revolutions of the counter drive gear as output shaft speed. These signals are transmitted to the TCM. Based on those signals, the TCM controls engine torque, shift timing, and TCC.

ac9uun00000819