ELECTRONIC CONTROL ITEMS AND CONTENTS [AY6A-EL, AY6AX-EL]

id0517k3223500

Item | Content
--- | ---
Driver adaptive shift control | • In D position, automatically switches between NORMAL, AAS, HIGH TEMP, CRUISE CONTROL, DOWN-SLOPE, UP-SLOPE, COLD modes according to specific conditions.
Manual mode shift control | • Shifts to selected gear position by manual shifting of the selector lever forward and back.
TCC, slip control | • According to preset TCC point, performs TCC operation via smooth TCC. • Slip control, by sliding the TCC when TCC is in the off range, extends the TCC range to low vehicle speeds.
Garage shift control | • Regulated oil pressure is supplied to the clutch when the selector lever is moved from N to D or from N to R, after the engine started.
Reverse control | • If the selector lever is moved from N to R while the vehicle is traveling and the transaxle shifts into reverse, TCM inhibits the transaxle from shifting into reverse while traveling.
Engine-transaxle total control | • Optimally controls engine output torque when shifting. • Operates optimal clutch engagement pressure corresponding to engine output torque.
On-board diagnostic system | • Detects and/or memorizes failure of input/output part and transaxle condition.