PARKING LIGHT BULB REMOVAL/INSTALLATION

id091800804200

1. Disconnect the negative battery cable.

2. When removing the parking light bulb on the right side, remove the coolant reserve tank first. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove in the order indicated in the table.

ac9wzw00002567

1 | Cover
2 | Socket
3 | Parking light bulb

4. Install in the reverse order of removal.