No.4 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW MAIN SWITCH [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]

id0903j4831300

4 | All power windows other than driver’s side do not operate using the power window main switch
POSSIBLE CAUSE | • Open or short circuit in wiring harness between ignition switch (IG1) and power window main switch (IG1). • Power window main switch malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ON position. • Set the power cut-switch to the UNLOCK position. • Operate all power windows other than the driver’s side using the power window main switch. • Do any power windows operate? | Yes | Replace the power window main switch. (See POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION.)
No | Inspect for an open or short circuit in the power window main switch wiring harness (battery power supply). Inspect the power window main switch connector connection. (damage/pulled-out pins, corrosion) Repair or replace if necessary.