SUNROOF SWITCH INSPECTION

id091500800300

1. Disconnect the negative battery cable.

2. Remove the intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

3. Remove the front map light. (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

4. Verify that the continuity between the sunroof switch terminals is as indicated in the table.

ac9wzw00001577

  • If not as specified, replace the sunroof switch. (See SUNROOF SWITCH REMOVAL/INSTALLATION.)

  ac9wzw00001578