REAR STABILIZER REMOVAL/INSTALLATION [4WD]

id0214008005a2

1. Remove the presilencer. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the presilencer insulator.

ac9uuw00001931

3. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION.)

4. Remove the rear ABS wheel-speed sensor. (See REAR ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION [4WD].)

5. Remove the rear coil spring. (See REAR COIL SPRING REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

ac9uuw00000995

1 | Rear stabilizer component (See Rear Stabilizer Component Removal Note.)
2 | Stabilizer bracket
3 | Bushing
4 | Rear stabilizer (See Rear Stabilizer Installation Note.)

Rear Stabilizer Component Removal Note

1. Support the rear differential using a jack.

ac9uuw00000988

2. Remove the rear differential mounting bracket (front) installation bolts.

ampjjw00003054

3. Tilt the rear differential towards the front.

4. Remove the rear stabilizer from through the gap between the rear differential and rear crossmember.

Rear Stabilizer Installation Note

1. Install the rear stabilizer so that the identification mark faces the right side of the vehicle.

ac9wzw00001089