POWER WINDOW MOTOR REMOVAL/INSTALLATION

id091200001400

Front

1. Fully lower the rear door glass.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove the bolts.

ac9wzw00000910

5. Remove the power window motor from the power window regulator.

6. Disconnect the power window motor connector.

7. Install in the reverse order of removal.

  Note
  • When installing the power window motor to the power window regulator drum, the drum housing tabs may detach from the door module. If this happens, insert a hand through the speaker installation hole to engage the drum housing tabs, and install the power window motor to the drum while supporting the drum housing.

Rear

1. Fully lower the rear door glass.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove the bolts.

ac9wzw00000911

5. Remove the power window motor from the power window regulator.

6. Disconnect the power window motor connector.

7. Install in the reverse order of removal.

  Note
  • When installing the power window motor to the power window regulator drum, the drum housing tabs may detach from the door module. If this happens, insert a hand through the speaker installation hole to engage the drum housing tabs, and install the power window motor to the drum while supporting the drum housing.