INSTRUMENTATION/DRIVER INFO. PERSONALIZATION FEATURES

id092200468400

• A personalization function has been adopted with which settings for each function can be changed.

Blind Spot Monitoring (BSM) System

Mazda Modular Diagnostic System (M-MDS) display | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
BSM buzzer | The operation of BSM warning alarm can be turned off. | Enabled | Disabled / Enabled | BSM control module

Lane Departure Warning System (LDWS)

LCD | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
FOW LDWS | The operation of LDWS and FOW can be turned off. | FOW ON/LDWS ON | FOW ON/LDWS ON, FOW ON/LDWS OFF, FOW OFF/LDWS ON, FOW OFF/LDWS OFF | Forward sensing camera (FSC)
LDWS Vol. | The volume of the LDWS warning alarm can be changed. | Hi | Hi / Lo | FSC
LDWS Sens. | The warning operation sensitivity of the LDWS can be changed. | Lo | Hi / Lo | FSC

Forward Obstruction Warning (FOW) System

LCD | Function | Initial setting | Setting contents | Control unit
--- | --- | --- | --- | ---
FOW LDWS | The operation of LDWS and FOW can be turned off. | FOW ON/LDWS ON | FOW ON/LDWS ON, FOW ON/LDWS OFF, FOW OFF/LDWS ON, FOW OFF/LDWS OFF | FSC
FOW Dist. | The warning operation distance of the FOW can be changed. | Near | Far / Near | FSC