CIGARETTE LIGHTER REMOVAL/INSTALLATION

id092000803100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See SELECTOR LEVER COMPONENT REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00000593

1 | Cigarette lighter plug
2 | Socket (See Socket Removal Note.)
3 | Ring (See Ring Removal Note.)

4. Install in the reverse order of removal.

Socket Removal Note

1. Remove the socket in the direction of the arrow (2) shown in the figure while opening the caps in the direction of the arrow (1) using a tape-wrapped fastener remover.

ac9wzw00000608

Ring Removal Note

1. Remove the ring in the direction of the arrow (2) shown in the figure while pressing the ring tabs in the direction of the arrow (1).

ac9wzw00000609