DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

id081000801300

  Warning
  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the air bag system service warnings and cautions before handling the air bag module. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)

1. Turn the ignition switch to the OFF position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove in the order indicated in the table.

L.H.D.

ac9wzw00000935

R.H.D.

ac9wzw00000936

1 | Cover
2 | Bolt
3 | Connector A (See Connector A Removal Note.)
4 | Connector B
5 | Driver-side air bag module

4. Install in the reverse order of removal.

5. Turn the ignition switch to the ON position.

6. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system. (See FLOWCHART.)

Connector A Removal Note

1. Using a flathead screwdriver, pry out the connector locking device.

ac9wzw00000937

2. Disconnect the connector.