IGNITER REMOVAL/INSTALLATION

id091800814200

  Warning
  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Disconnect the negative battery cable.

2. When removing the igniter on the right side, remove the coolant reserve tank first. (See COOLANT RESERVE TANK REMOVAL/INSTALLATION [MZI-3.7].)

3. Rotate the cover in the direction of the arrow (1) shown in the figure and remove it from the front combination light in the direction of the arrow (2) shown in the figure.

ac9wzw00002575

4. Rotate the igniter in the direction of the arrow (3) shown in the figure and remove it from the front combination light in the direction of the arrow (4) shown in the figure.

ac9wzw00002576

5. Insert the flathead screwdriver into the gap between the igniter and connector shown in the figure.

ac5wzw00001210

6. Move the flathead screwdriver in the direction of the arrow (5) shown in the figure, lift up the connector, and disconnect it.

ac9wzw00002577

7. Install in the reverse order of removal.