LIFTGATE LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION

id091400803800

Vehicles With PLG

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

ac9wzw00001917

1 | Bolt
2 | Connector
3 | Liftgate latch and lock actuator

6. Install in the reverse order of removal.

Vehicles Without PLG

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the liftgate side trim. (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

ac9wzw00001918

1 | Bolt
2 | Connector
3 | Cable
4 | Liftgate latch and lock actuator

6. Install in the reverse order of removal.