REVERSE CONTROL OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3226300

• If the selector lever is moved from N to R while the vehicle is traveling and the transaxle shifts into reverse, the wheels may be locked, which is extremely dangerous. In order to avoid this, TCM inhibits the transaxle from shifting into reverse while traveling.

  Note
  • Even when the selector lever is moved from N to R, the transaxle does not shift into reverse if the vehicle speed is 11 km/h {6.9 mph} or more.
  • When this control is activated, the C3 clutch is released with operating the shift solenoid E so that the transaxle does not shift into reverse.
  • Reverse control takes precedence over N-R shift control.