DTC INSPECTION [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7345400

1. Turn the ignition switch to the OFF position.

  Caution
  • Perform the procedure in Steps 2 to 3 within 30 s.

2. Turn the ignition switch to the ON position.

  Note
  • The DTCs are output after about 10 s from when the ignition switch is turned to the ON position.

3. Connect terminals B (INIT) and J (GND) of the DLC-2 using a jumper wire.

  Caution
  • If the terminals are mistakenly connected, vehicle damage or fire could occur. When connecting with the jumper wire, thoroughly verify what terminals are being connected to prevent a miss-connection.

L.H.D

ac9wzw00001419

R.H.D

ac9wzw00001420

4. Read the DTCs by the flashing pattern of the headlight auto leveling warning light.

ac9wzw00001421

5. After verifying the DTCs. pull out the jumper wire from DLC-2.