PCM REMOVAL/INSTALLATION [MZI-3.7]

id0140c3802400

  Note
  • For replace the PCM, setup the M-MDS and perform the PCM configuration. (See PCM CONFIGURATION [MZI-3.7].)

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

3. Disconnect the PCM connectors.

4. Remove the PCM and bracket as assembly.

ac9wzw00001733

5. Remove in the order indicated in the table.

ac9wzw00002363

1 | PCM bracket No.1
2 | PCM
3 | PCM bracket No.2

6. Install in the reverse order of removal.

7. When replacing the PCM on the vehicles, perform the following:

  • PCM parameter reset (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [ADVANCED KEYLESS ENTRY AND START SYSTEM].)(See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [KEYLESS ENTRY SYSTEM].)