DRIVELINE/AXLE TECHNICAL DATA

id035000800100

Front and Rear Axle

Item | Specification
--- | ---
Front wheel bearing maximum play | 0.05 mm {0.002 in}
Rear wheel bearing maximum play | 0.05 mm {0.002 in}

Drive Shaft

Item | Specification
--- | ---
Front drive shaft standard length | LH: 658.7—668.7 mm {25.92—26.30 in} RH: 630.7—640.7 mm {24.82—25.20 in}
Rear drive shaft standard length | Crimped-fix locknut type: LH: 840.3—850.3 mm {33.09—33.47 in} RH: 895.3—905.3 mm {35.25—35.64 in} Self-locking nut type: LH: 842.3—852.3 mm {33.17—33.55 in} RH: 897.3—907.3 mm {35.33—35.72 in}

Differential

Item | Specification
--- | ---
Rear differential oil | Specified oil grade: API service GL-5 Specified oil viscosity: SAE 80W-90 Capacity (approx quantity): 1.0 L {1.1 US qt, 0.9 Imp qt}
Rear differential backlash of pinion gear and side gear | 0.1 mm {0.004 in} or less
Rear differential pinion height | -0.032—0.032 mm {-0.0012—0.0012 in}
Rear differential drive pinion preload | 1.3—1.8 N·m {14—18 kgf·cm, 12—15 in·lbf}
Rear differential backlash of drive pinion and ring gear | Standard: 0.09—0.11 mm {0.003—0.004 in} Minimum value: 0.05 mm {0.002 in}

Propeller Shaft

Item | Specification
--- | ---
Propeller shaft maximum runout | 0.8 mm {0.031 in}
Propeller shaft starting torque | 0.29—1.47 N·m {3.0—14.9 kgf·cm, 2.6—13.0 in·lbf}

Transfer

Item | Specification
--- | ---
Transfer oil | Type | Grade | API service GL-5
Viscosity | SAE 75W-140
Oil capacity (approx. quantity) | (L {US qt, Imp qt}) | 0.53 {0.56, 0.47}