FRONT DOOR GLASS REMOVAL/INSTALLATION

id091200000100

1. To access the glass installation bolt, position the front door glass so that the distance from the top of the front door glass to the upper part of the front beltline molding is approx. 120 mm {4.72 in}.

ac9uuw00002334

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove the hole cover.

ac9wzw00001613

5. Remove the bolts.

6. Lift the front door glass up and remove it in the direction of the arrow.

ac9wzw00001614

7. Install in the reverse order of removal.

  Note
  • When installing the front door glass, align the glass edge with the glass run channel by hand through the speaker installation hole.