FAIL-SAFE OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3226600

• With the fail-safe function, if any malfunction should occur in the automatic transaxle system, the TCM will output a control signal, and control will be performed to make traveling a minimum distance possible. If a shift solenoid malfunction, the TCM will cancel the output of control signals to the solenoid. If this happens, oil pressure circuits alone will control automatic transaxle gear shifting. The gears will shift as shown in the chart below.

Shift position | Gear position
--- | ---
R | Reverse
D, M | 3rd gear (5th gear in case of shift solenoid C malfunction)