VENTILATOR GRILLE REMOVAL/INSTALLATION

id091700804600

Driver Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Upper column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Remove the screws.

ac9uuw00000347

4. Remove the hook.

5. Remove the ventilator grille in the direction of the arrow.

6. Install in the reverse order of removal.

Passenger Side

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (6) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (7) Dashboard garnish (See DASHBOARD GARNISH REMOVAL/INSTALLATION.)

3. Remove the screws.

ac9uuw00000348

4. Remove the hook.

5. Remove the ventilator grille in the direction of the arrow.

6. Install in the reverse order of removal.

Center

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (2) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (3) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

3. Remove the screws

ac9uuw00000349

4. Remove the ventilator grille.

5. Install in the reverse order of removal.

Rear

1. Disconnect the negative battery cable.

2. Remove the console cover. (See CONSOLE COVER REMOVAL/INSTALLATION.)

3. Remove the rear cooler duct. (See REAR COOLER DUCT REMOVAL/INSTALLATION.)

4. Detach the pins A while holding the console cover.

ac9uuw00000606

5. Remove the ventilator grille in the direction of the arrow.

6. Install in the reverse order of removal.