SEAT BELT WARNING ALARM CONSTRUCTION/OPERATION

id092200101800

System Wiring Diagram

ac9wzn00000414

Operation

• The buzzer in the instrument cluster sounds for 32—34 s when all the following two conditions are met:

  ― The seat belt (driver side or passenger side) is unfastened (driver side: buckle switch is on, front passenger side: buckle switch is on).
  ― The vehicle speed is 15—20 km/h {9.4—12.0 mph} or more.