TRANSMISSION/TRANSAXLE SPECIFICATIONS

id050000302100

Automatic Transaxle [AY6A-EL, AY6AX-EL]

Item | Specifications
--- | ---
Engine type | MZI-3.7
Gear ratio | 1GR | 4.148
2GR | 2.370
3GR | 1.555
4GR | 1.154
5GR | 0.859
6GR | 0.685
Reverse | 3.393
Final gear ratio | 3.464
ATF | Type | JWS3309
Capacity (Approx. quantity) | (L {US qt, lmp qt}) | 6.6 {7.0, 5.8}
Torque converter stall torque ratio | 1.97
Hydraulic system (Number of drive/driven plates) | C1 clutch | 7/7
C2 clutch | 4/4
C3 clutch | 4/4
B2 brake | 6/5
Band servo | Servo diameter (Piston outer dia./retainer outer dia.) | (mm {in}) | 61.3/66.0 {2.41/2.60}
Front planetary gear (Number of teeth) | Ring gear | 81
Sun gear | 45
Pinion gear | 17
Rear planetary gear (Number of teeth) | Ring gear | 72
Middle sun gear | 33
Rear sun gear | 27
Long pinion gear | 18
Short pinion gear | 17
Counter drive gear (Number of teeth) | 51
Counter gear (Number of teeth) | Driven gear | 50
Drive gear | 15
Ring gear (Number of teeth) | 53