FRONT DOOR KEY CYLINDER REMOVAL/INSTALLATION

id091400429400

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Front door module (See FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00001144

1 | Rod
2 | Bolt
3 | Front door key cylinder (See Front Door Key Cylinder Removal Note.)

4. Install in the reverse order of removal.

Front Door Key Cylinder Removal Note

1. Remove the front door key cylinder by turning it in the direction shown by the arrow.

ac9wzw00001924