AUTO LIGHT-OFF SYSTEM OPERATION

id091800106200

Operation

• When the following conditions are satisfied, the auto light/wiper control module turns on the lights and activates the built-in timer. When the specified time has passed, the lights go off.

Condition before operation | Operation condition | Illumination time
--- | --- | ---
• Ignition switch is at ON position. • Light switch is at TNS or HEAD position. • Light switch is in AUTO position and auto light system is operating. | Ignition switch is turned to OFF or ACC position. | Approx. 30 s
• Ignition switch is at OFF or ACC position. | Light switch is turned to TNS or HEAD position.
• Light switch is at TNS position and timer is operating. • Light switch is at AUTO position and timer is operating. | Light switch is turned to HEAD position.

• The timer is canceled according to the following conditions, and then the system operates as follows:

Cancel condition | Auto light-off system operation
--- | ---
Ignition switch is turned to ON position. | • When light switch is at TNS position, TNS relay turns on. • When light switch is at HEAD position, headlight relay (LO) and TNS relay turns on.
Light switch is turned off. | TNS and headlight relay (LO) turn off.
Light switch is turned AUTO position. | TNS and headlight relay (LO) turn off.

• The lights turn on when the ignition switch is at the ON position and the light switch is at the TNS or HEAD position, even if the auto light/wiper control module is malfunctioning.

Timing Chart

ac9wzn00000584