FRONT DRAIN HOSE REMOVAL

id091500801300

1. Disconnect the negative battery cable.

2. Partially peel back the seaming welt.

3. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (6) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (8) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (9) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (14) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (15) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (18) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (19) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (20) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (21) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (22) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (23) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

  (24) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (25) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (26) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (27) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (28) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (29) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (30) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (31) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (32) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (33) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (34) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (35) Bonnet release lever (See BONNET REMOVAL/INSTALLATION.)

  (36) Fuel-filler lid release lever (R.H.D.) (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

  (37) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (38) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (39) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (40) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (41) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (42) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (43) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (44) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (45) Audio unit (vehicles with audio system) (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (46) Car-navigation unit (vehicles with car-navigation system) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (47) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (48) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (49) Dashboard (See DASHBOARD REMOVAL/INSTALLATION.)

4. Disconnect the front drain hose from the sunroof frame.

5. Remove the front drain hose from the clips.

ac9wzw00001574

6. Pull the front drain hose into the room side.

7. Remove the front drain hose.