FRONT DOOR MODULE PANEL REMOVAL/INSTALLATION

id091100520200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)

  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)

3. Disconnect the power outer mirror connector.

4. Remove the clips securing the wiring harness shown in the figure and set the wiring harness out of the way.

ac9wzw00000851

5. Remove screws and fastener.

ac9wzw00000852

6. Remove the front door module panel.

7. Install in the reverse order of removal.