BLIND SPOT MONITORING (BSM) INDICATOR LIGHT INSPECTION

id092200645100

1. Disconnect the negative battery cable.

2. Remove the inner garnish. (See INNER GARNISH REMOVAL/INSTALLATION.)

ac9uuw00003436

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Apply battery voltage to power outer mirror terminal D, and terminal G to ground.

  • Verify that the BSM indicator light illuminates.

5. Remove the outer mirror glass. (See OUTER MIRROR GLASS REMOVAL.) (See OUTER MIRROR GLASS INSTALLATION.)

6. Apply battery voltage to BSM indicator light terminal A, and terminal B to ground.

acxuuw00004179

  • Verify that the BSM indicator light illuminates. If there is any malfunction, replace the BSM indicator light. (See BLIND SPOT MONITORING (BSM) INDICATOR LIGHT REMOVAL/INSTALLATION.)

7. Inspect for continuity between the following terminals:

ac9uuw00003437

  • Power outer mirror terminal D—BSM indicator light terminal A
  • Power outer mirror terminal G—BSM indicator light terminal B
    ― If not as indicated in the table, replace the power outer mirror.

ac9uuw00003438