FRONT EVAPORATOR TEMPERATURE SENSOR INSPECTION

id074000804100

1. Set the fan speed MAX HI.

2. Set the temperature control at MAX COLD.

3. Set the RECIRCULATE mode.

4. Turn the A/C switch off.

5. Close all doors and windows.

6. Wait for 5 min.

7. Remove the glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

8. Disconnect the front evaporator temperature sensor connector.

9. Measure the temperature at the blower inlet.

10. Measure the resistance between the front evaporator temperature sensor terminals.

am8rrw00000822

  • If the resistance is not as shown in the graph, replace the front evaporator temperature sensor.