IGNITION KEY ILLUMINATION BULB REMOVAL/INSTALLATION

id091800802400

Vehicles Without Advanced Keyless System

1. Disconnect the negative battery cable.

2. Pull the upper column cover upward and detach the upper column cover from the lower column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

3. Put aside the upper column cover.

4. Remove the ignition key illumination bulb.

am8rrw00001225

5. Install in the reverse order of removal.