COURTESY LIGHT BULB REMOVAL/INSTALLATION

id091800808100

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

ampjjw00002945

1 | Lens (See Lens Removal Note.)
2 | Courtesy light bulb

3. Install in the reverse order of removal.

Lens Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole and pry with the screwdriver in the direction shown by the arrow to remove the lens.

am8rrw00001218