NO.11 SHIFT POINT IS HIGH OR LOW [AY6A-EL, AY6AX-EL]

id0503k3801600

11 | Shift point is high or low
DESCRIPTION | • Shift point considerably different from automatic shift diagram. • Shift delays when accelerating. • Shift occurs quickly when accelerating and engine speed does not increase.
POSSIBLE CAUSE | • If the transaxle does not shift abnormally, there is a malfunction of the input signal to the APP sensor, input/turbine speed sensor, or VSS. • If the engine speed is high or low, regardless of normal shifting, inspect the tachometer. • Verify that the output signals of the APP sensor change linearly. Note • If a tire of a different diameter from the standard tire is installed, the TCM determines that the driving mode is the AAS mode, and may change to a different shift timing from the normal timing.