ON-BOARD DIAGNOSTIC SYSTEM SIMULATION FUNCTION [MZI-3.7]

id0102d2142200

Features

• Simulation items for output components are supported.

Function

• Output parts preset in the PCM can be operated regardless of PCM control status.
• The items that can be operated are as shown below.

Active command mode table

Item | Applicable component | Unit/condition
--- | --- | ---
ACCS | A/C relay | Off/On
ARPMDES | Target engine speed | RPM
EVAPCP | Purge solenoid valve duty value | %
EVAPCV | Evaporative emission canister vent valve | Off/On
FAN_DUTY | Variable fan duty cycle | %
FP | Fuel pump relay | Off/On
INJ_1 | Fuel injector No.1 | OFF
INJ_2 | Fuel injector No.2 | OFF
INJ_3 | Fuel injector No.3 | OFF
INJ_4 | Fuel injector No.4 | OFF
INJ_5 | Fuel injector No.5 | OFF
INJ_6 | Fuel injector No.6 | OFF