COWL PANEL REMOVAL/INSTALLATION

id091000802000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION)

  (2) Cowl grille (See COWL GRILLE REMOVAL/INSTALLATION)

  (3) Windshield wiper motor (See WINDSHIELD WIPER MOTOR REMOVAL/INSTALLATION)

3. Remove the bolts, then remove the cowl panel.

ac9wzw00002500

4. Install in the reverse order of removal.