MASTER CYLINDER REMOVAL/INSTALLATION [L.H.D.]

id041100801350

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

2. Remove the resonance chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

3. Remove the bolt and nut as shown in the figure, and move the vacuum pipe bracket.

ac9wzw00001760

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. After installation, add brake fluid, bleed the air, and inspect for fluid leakage. (See AIR BLEEDING.)

ac9wzw00003279

1 | Brake fluid level sensor connector
2 | Brake pipe
3 | Master cylinder component
4 | O-ring