ACTIVE COMMAND MODES TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0902q2960900

Command name | Operation condition | Unit/Operation | Output part name
--- | --- | --- | ---
BSM_OFF_IL*2 | • BSM OFF indicator light turns off: Off • BSM OFF indicator light illuminates: On | Off/On | BSM OFF indicator light
Buzzer*2 | • Buzzer stops: Off • Buzzer sounds: On | Off/On | Buzzer
WRN_IND_L*1 | • BSM indicator light (LH) turns off: Off • BSM indicator light (LH) illuminates: On | Off/On | BSM indicator light (LH)
WRN_IND_R*2 | • BSM indicator light (RH) turns off: Off • BSM indicator light (RH) illuminates: On | Off/On | BSM indicator light (RH)
VSPD | • Cancel inputting the vehicle speed: OFF • Input the vehicle speed of 34 km/h {21 mph}: ON | OFF/ON | Vehicle speed

*1 :BSM control module (LH)
*2 :BSM control module (RH)